

HW6 – figures







Boundary fluxes – base case







Head profiles and flow map – base case – area affected by recharge contamination




Plots of ET, recharg and water table depth for base case.



Fluxes and ET after extinction depth changed to 2 instead of 3




Boundary fluxes after extinction depth changed to 2







Head countours and flow map for extinction depth of 2





Head profile and flow map for well pumping case – contamination zone highlighted.





ET, recharge, and WTD for well pumping case

Water balance numbers for well recharge case.